{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Name","Gewicht (g)","Preis $","Preis €"]
["Modell",null,null,null,0]
["Servo1",null,null,null,0]
["Servo2",null,null,null,0]
["Motor",null,null,null,0]
["Regler",null,null,null,0]
["Empfänger",null,null,null,0]
["Akku",null,null,null,0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
["Total:",null,0,0,0]
{"$rows_empty":7}
["Lipos:","Zelle","Kapazität","Gewicht (g)","C","max. Strom","Maße"]
[null,"HXT 60",60,1.9,"12",720,"13x16x4.4mm"]
[null,"HXT 100",100,"3,4",12,1200,"16x29x3mm"]
[null,"HXT 135",135,4,12,1620,"21x30x3mm"]
[null,"HXT 180",180,5.1,12,2160,"22x31x4.1mm"]
[null,"HXT 200",200,6.2,12,2400,"31x20x4mm"]
[null,"HXT 250",250,7.2,12,3000,"50x30x2.2mm"]
[null,"HXT 300",300,7,12,3600,"37x22x4mm"]
[null,"HXT 450",450,12.5,12,5400,"50x30x3.5mm"]
[null,"ZIPPY240S20C",240,5.9,20,4800,"35x21x5.3mm"]
[]
["Servos:","Modell","Gewicht (g)","Maße"]
[null,"EM_37g",4.3,"19x8x26mm"]
[null,"EM_37g stripped",3.2,"19x8x26mm"]
[null,"EM_43g",4.9,"19x8x26mm"]
[null,"HXT500",5,"22.9x11.4x22 mm"]
[null,"HXT900",9,"21x12x22 mm"]
[]
[]
["Empfänger:","RS410",4.9]
[null,"RS410 stripped",3.2]
[null,"Micro Bidproduct",2.3]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}